One router configuration

|  |
| --- |
| Router>en  Router#conf t  Enter configuration commands, one per line. End with CNTL/Z.  Router(config)#interface fastEthernet 0/0  Router(config-if)#ip address 192.168.1.1 255.255.255.0  Router(config-if)#no shutdown  Router(config-if)#  %LINK-5-CHANGED: Interface FastEthernet0/0, changed state to up  %LINEPROTO-5-UPDOWN: Line protocol on Interface FastEthernet0/0, changed state to up  Router(config-if)#ip dhcp pool ice  Router(dhcp-config)#network 192.168.1.0 255.255.255.0  Router(dhcp-config)#default-router 192.168.1.1  Router(dhcp-config)#  Router(dhcp-config)#exit  Router(config)#exit  Router#  %SYS-5-CONFIG\_I: Configured from console by console  Router#wr  Building configuration...  [OK]  Router#conf t  Enter configuration commands, one per line. End with CNTL/Z.  Router(config)#interface fastEthernet 0/1  Router(config-if)#ip address 192.168.2.1 255.255.255.0  Router(config-if)#no shutdown  Router(config-if)#  %LINK-5-CHANGED: Interface FastEthernet0/1, changed state to up  %LINEPROTO-5-UPDOWN: Line protocol on Interface FastEthernet0/1, changed state to up  Router(config-if)#ip dhcp pool VLAN2  Router(dhcp-config)#network 192.168.2.0 255.255.255.0  Router(dhcp-config)#default-router 192.168.2.1  Router(dhcp-config)#exit  Router(config)#ex  Router#  %SYS-5-CONFIG\_I: Configured from console by console  Router#wr  Building configuration...  [OK]  Router# |